Copyright © 2019 Apple Inc.

The files in this folder consist of SDR P3 DCI primaries and secondaries at 100% saturation and 100% amplitude.

The theoretical (ideal) luminance and CIE 1931 x,y for Digital Cinema (P3-DCI) reference mode are:

P3 DCI          x       y         cd/m^2
Red             0.6800  0.3200    10.06
Green           0.2650  0.6900    34.64
Blue            0.1500  0.0600    3.31
Cyan            0.2048  0.3602    37.94
Magenta         0.3424  0.1544    13.36
Yellow          0.4248  0.5476    44.69